From ad492666069444a9ebc0c8fdf115375acf064c3f Mon Sep 17 00:00:00 2001
From: Stephen Hemminger <shemminger@vyatta.com>
Date: Thu, 11 Aug 2011 14:56:19 -0700
Subject: Don't bring ethernet device up if it is disabled

If ethernet (or pseudo) is disabled, don't bounce link.
---
 templates/interfaces/ethernet/node.def | 4 +++-
 1 file changed, 3 insertions(+), 1 deletion(-)

(limited to 'templates/interfaces/ethernet/node.def')

diff --git a/templates/interfaces/ethernet/node.def b/templates/interfaces/ethernet/node.def
index 426f8f87..45d6ec09 100644
--- a/templates/interfaces/ethernet/node.def
+++ b/templates/interfaces/ethernet/node.def
@@ -20,7 +20,9 @@ begin: rm -f /tmp/speed-duplex.$VAR(@)
              --set-mac "$VAR(mac/@)"
        fi
 
-create: ip link set "$VAR(@)" up
+create: if ! cli-shell-api exists interfaces ethernet $VAR(@) disable;
+	then ip link set $VAR(@) up
+	fi
 	/opt/vyatta/sbin/vyatta-link-detect $VAR(@) on
 
 delete: [ -d /sys/class/net/$VAR(../@) ] || exit 0
-- 
cgit v1.2.3

