type: u32
help: Set initial hold time(msec) between consecutive SPF calculations
default: 1000
syntax:expression: $VAR(@) >= 0 && $VAR(@) <= 600000; "must be between 0-600000"
comp_help: possible completions:
 <0-600000>         Initial hold time in msec (default 1000)
