type: u32
default: 180
help: Routing information timeout timer
val_help: u32:0-65535; Routing information timeout timer (default 180)

syntax:expression: $VAR(@) >= 0 && $VAR(@) <= 65535; \
       "Timeout timer must be between 0 and 65535"
