From ad492666069444a9ebc0c8fdf115375acf064c3f Mon Sep 17 00:00:00 2001
From: Stephen Hemminger <shemminger@vyatta.com>
Date: Thu, 11 Aug 2011 14:56:19 -0700
Subject: Don't bring ethernet device up if it is disabled

If ethernet (or pseudo) is disabled, don't bounce link.
---
 templates/interfaces/pseudo-ethernet/node.def | 7 ++++++-
 1 file changed, 6 insertions(+), 1 deletion(-)

(limited to 'templates/interfaces/pseudo-ethernet/node.def')

diff --git a/templates/interfaces/pseudo-ethernet/node.def b/templates/interfaces/pseudo-ethernet/node.def
index 5b0aaac9..4f8510f3 100644
--- a/templates/interfaces/pseudo-ethernet/node.def
+++ b/templates/interfaces/pseudo-ethernet/node.def
@@ -6,9 +6,14 @@ val_help: <pethN>; Pseudo Ethernet interface name
 
 syntax:expression: pattern $VAR(@) "^peth[0-9]+$" \
          ; "name must be (peth0-peth999)"
+
 commit:expression: $VAR(link) != "" 
          ; "link device must be set for virtual ethernet $VAR(@)"
+
 create:	ip link add $VAR(@) link $VAR(link/@) type macvlan || exit 1
-	ip link set $VAR(@) up
+	if ! cli-shell-api exists interfaces ethernet $VAR(@) disable;
+	then ip link set $VAR(@) up
+	fi
 	/opt/vyatta/sbin/vyatta-link-detect $VAR(@) on
+
 delete: ip link delete dev $VAR(@) type macvlan
-- 
cgit v1.2.3

