type: ipv4
help: Local RADIUS client address from which packets are sent
