type: u32
help: Time interval between heartbeat packets (milliseconds)
default: 5000
