type: u32
help: Interval after which a monitor node is considered dead (milliseconds)
default: 20000
