help: Monitor Network Address Translation (NAT)
run: ${vyatta_bindir}/vyatta-monitor NAT "\[NAT-[0-9]*-*\]"
