From d3366af025f4698801c0a51cdd9bbb88fea83ea0 Mon Sep 17 00:00:00 2001
From: Stephen Hemminger <stephen.hemminger@vyatta.com>
Date: Tue, 20 Jul 2010 10:04:41 -0700
Subject: Convert interface templates to use val_help:

---
 interface-templates/ip/ospf/priority/node.def | 6 +++---
 1 file changed, 3 insertions(+), 3 deletions(-)

(limited to 'interface-templates/ip/ospf/priority/node.def')

diff --git a/interface-templates/ip/ospf/priority/node.def b/interface-templates/ip/ospf/priority/node.def
index bd59276c..f7f83d94 100644
--- a/interface-templates/ip/ospf/priority/node.def
+++ b/interface-templates/ip/ospf/priority/node.def
@@ -1,8 +1,8 @@
 type: u32
-help: Set router priority
+help: Router priority
 default: 1
 syntax:expression: $VAR(@) >= 0 && $VAR(@) <= 255; "Must be between 0-255"
+val_help: u32:0-255; Priority (default 1)
+
 update:vtysh -c "configure terminal" -c "interface $IFNAME" -c "ip ospf priority $VAR(@)"
 delete:vtysh -c "configure terminal" -c "interface $IFNAME" -c "no ip ospf priority"
-comp_help: possible completions:
- <0-255>            Priority (default 1)
-- 
cgit v1.2.3

