From 2f6ceb414f9c45bb98505d2773f077c243e13e59 Mon Sep 17 00:00:00 2001
From: slioch <slioch@eng-140.vyatta.com>
Date: Thu, 19 Feb 2009 20:32:10 -0800
Subject: applied same changes to ospf and rip as to bgp re: start/stop router
 daemon hooks

---
 templates/protocols/rip/node.def | 3 ++-
 1 file changed, 2 insertions(+), 1 deletion(-)

(limited to 'templates/protocols/rip/node.def')

diff --git a/templates/protocols/rip/node.def b/templates/protocols/rip/node.def
index b7f085a5..2c2d300c 100644
--- a/templates/protocols/rip/node.def
+++ b/templates/protocols/rip/node.def
@@ -1,5 +1,6 @@
 help: Configure Routing Information Protocol (RIP) parameters
-begin: sudo /opt/vyatta/sbin/quagga-manager start ripd
+create: sudo /opt/vyatta/sbin/quagga-manager start ripd
 create: vyatta-vtysh -c "configure terminal" -c "router rip"
 delete: vyatta-vtysh -c "configure terminal" -c "no router rip"
+delete: sudo /opt/vyatta/sbin/quagga-manager stop ripd
 end: sudo /opt/vyatta/sbin/quagga-manager update
-- 
cgit v1.2.3

