type: u32
help: Set router priority
default: 1
syntax:expression: $VAR(@) >= 0 && $VAR(@) <= 255; "Must be between 0-255"
update:vyatta-vtysh -c "configure terminal" -c "interface $IFNAME" -c "ip ospf priority $VAR(@)"
delete:vyatta-vtysh -c "configure terminal" -c "interface $IFNAME" -c "no ip ospf priority "
comp_help: possible completions:
 <0-255>            Priority (default 1)
