type: u32
help: Set link state transmit delay
default: 1
syntax:expression: $VAR(@) >= 1 && $VAR(@) <= 65535; "Must be between 1-65535"
update:vtysh -c "configure terminal" -c "interface $IFNAME" -c "ip ospf transmit-delay $VAR(@)"
delete:vtysh -c "configure terminal" -c "interface $IFNAME" -c "no ip ospf transmit-delay"
comp_help: possible completions:
 <1-65535>          Seconds (default 1)
