tag:
priority: 310
type: txt
help: Bridge interface name
comp_help: "Enter bridge interface name (br0 - br999)"

syntax:expression: pattern $VAR(@) "^br[0-9]+$" ; "Must be (br0 - br999)"

create: /usr/sbin/brctl addbr $VAR(@)
        ip link set $VAR(@) up

delete: if ! /opt/vyatta/sbin/vyatta-bridgegroup-depedency.pl   \
          --no-interfaces-assigned                            	\
          --bridge-interface="$VAR(@)"; then                    \
          exit 1
        fi
        ip link set $VAR(@) down;
        /usr/sbin/brctl delbr $VAR(@);

