tag:
priority: 390
type: txt
help: Set Pseudo Ethernet device name
comp_help: Enter Pseudo Ethernet interface name (peth0 - peth999)
syntax:expression: pattern $VAR(@) "^peth[0-9]+$" \
         ; "name must be (peth0-peth999)"
commit:expression: $VAR(link) != "" 
         ; "link device must be set for virtual ethernet $VAR(@)"
create:	sudo ip link add $VAR(@) link $VAR(link/@) type macvlan || exit 1
	sudo ip link set $VAR(@) up
	/opt/vyatta/sbin/vyatta-link-detect $VAR(@) on
delete: sudo ip link delete dev $VAR(@) type macvlan
