type: u32
help: Set refresh timer
syntax:expression: $VAR(@) >= 10 && $VAR(@) <= 1800; "must be between 10-1800"
update: ${vyatta_sbindir}/vyatta-vtysh.pl -c "configure terminal" \
          -c "router ospf"                                        \
          -c "no refresh timer" -c "refresh timer $VAR(@)"; 
delete: ${vyatta_sbindir}/vyatta-vtysh.pl -c "configure terminal" \
          -c "router ospf"                                        \
          -c "no refresh timer $VAR(@)";
comp_help: possible completions:
  <10-1800>          Timer value in seconds
